*LIGO Laboratory / LIGO Scientific Collaboration*

LIGO- E200627-v1 Advanced LIGO 6/7/2012

TwinCAT Library for
Delay Line

Alexa Staley, Daniel Sigg

Distribution of this document:

LIGO Scientific Collaboration

This is an internal working note
of the LIGO Laboratory.

|  |  |
| --- | --- |
| **California Institute of Technology****LIGO Project – MS 18-34****1200 E. California Blvd.****Pasadena, CA 91125**Phone (626) 395-2129Fax (626) 304-9834E-mail: info@ligo.caltech.edu | **Massachusetts Institute of Technology****LIGO Project – NW22-295****185 Albany St****Cambridge, MA 02139**Phone (617) 253-4824Fax (617) 253-7014E-mail: info@ligo.mit.edu |
| **LIGO Hanford Observatory****P.O. Box 159****Richland WA 99352**Phone 509-372-8106Fax 509-372-8137 | **LIGO Livingston Observatory****P.O. Box 940****Livingston, LA 70754**Phone 225-686-3100Fax 225-686-7189 |

http://www.ligo.caltech.edu/

|  |
| --- |
| **Library** |
| Title | DelayLinePhaseShifter |
| Version | 1 |
| TwinCAT version | 2.11 |
| Name space | – |
| Author | Alexa Staley, Daniel Sigg |
| Description | The delay line shifter delays an input signal by a selectable amount. This amount can be controlled by a step or phase slider. The delay can be between 0ns and 30.762ns.  |
| Error Codes | 0x01 – Invalid frequency |
| Library dependencies | Error |

|  |
| --- |
| **Hardware Output Type**TYPE DelayLogicOutStruct :STRUCT DelayStep: INT;LacthEn: BOOL; END\_STRUCTEND\_TYPE |
| Type name | DelayLogicOutStruct |
| Description | Structure of the hardware output that are wired up for the delay line |
| Definition | STRUCT |
| Element | Name: DelayStepType: INTDescription: The delay line step slider |
| Element | Name: LatchEnType: BOOLDescription: Enables latch |

|  |
| --- |
| **User Interface Type**TYPE DelayLogicStruct :STRUCTFreqMhz: LREAL;PhaseDeg: LREAL;DelayNs: LREAL;DelayStep: INT;Error: ErrorStruct;END\_STRUCTEND\_TYPE |
| Type name | DelayLogicStruct |
| Description | Structure of the user interface tags that are used to control the delay line |
| Definition | STRUCT |
| Output Tag | Name: ErrorType: ErrorStructDescription: For error handling |
| Input Tag | Name: FreqMhzType: LREALDescription: Input frequency in MHz |
| In/out Tag | Name: PhaseDegType: LREALDescription: Input phase in degrees |
| In/out Tag | Name: DelayNsType: LREALDescription: Delay of input signal in nanoseconds |
| In/out Tag | Name: DelayStepType: INTDescription: Delay between 0ns and 31.9375ns can be added in steps |

|  |
| --- |
| **Function Block**FUNCTION\_BLOCK DelayLogicFBVAR\_INPUTEND\_VARVAR\_OUTPUTDelayLogicOut: DelayLogicOutStruct;END\_VARVAR\_IN\_OUT DelayLogic: DelayLogicStruct;END\_VAR |
| Name | DelayLogicFB |
| Description | Controls the delay line  |
| Output argument | Name: DelayLogicOutType: DelayLogicOutStructDescription: Output hardware structure |
| In/out argument | Name: DelayLogicType: DelayLogicStructDescription: User Interface structure |

|  |
| --- |
| **Visual** |
| Name | DelayLogicVis |
| Description | Displays phase, steps, and delay |
| Placeholder | Name: DelayLogicType: DelayLogicStructDescription: Delay Line structure |