*LIGO Laboratory / LIGO Scientific Collaboration*

LIGO-T12xxxxx-v1 *LIGO* Date 5/30/13

Getting wafers in/out of vertical holders

Margot

Distribution of this document:

LIGO Scientific Collaboration

This is an internal working note

of the LIGO Laboratory.

|  |  |
| --- | --- |
| **California Institute of Technology**  **LIGO Project** | **Massachusetts Institute of Technology**  **LIGO Project** |
| **LIGO Hanford Observatory** | **LIGO Livingston Observatory** |

http://www.ligo.caltech.edu/

# Introduction

This is a quick note on how to get the wafers in and out of the vertical wafer holders most easily, especially when removing them from the chamber, as we want to keep all the dust on their surfaces intact.

# Notes

Once the wafer holder has been placed on the table, it should not be moved around. Since it is vertical, any movement of the holder will probably knock off the particulate that you are trying to measure.

When ready to remove the whole thing from chamber, remove the screws holding it to the table then turn the wafer horizontal for transporting out of chamber. Very important to keep the shiny “Dust Accumulation” side **UP**.

# Pictures

These are pictures of removing a wafer. For placing one, do this in reverse. The wafer is laid on its side, again shiny “Dust Accumulation” side **UP**, screws are removed and the wafer is taken out with tweezers.



