MEMORANDUM

LIGO HANFORD OBSERVATORY

PO BOX 159

RICHLAND WA 99352

TEL: 509.372.8190

FAX: 509.372.8137

DATE: December 16, 2021

|  |  |
| --- | --- |
| TO: | ISC team |
| FROM: | Daniel Sigg |
| SUBJECT: | Modifications to the VCO source boards (initial build) |
| Refer to: | LIGO-E2100544-v1 |

Version 3 of VCO source boards, , as originally built, need the following modifications to reduce oscillations in the low noise power supply units.

Capacitors need to be NP0/COG or film, resistors need to be metal film.

Change 1:

Add improved compensation to PVCO supply.

R69 → 15 Ω
C112 → 470 pF

Change 2:

Add improved compensation to P20 supply.

R70 → 15 Ω
C113 → 470 pF
C93 → 2.2 µF

Change 3:

Add improved compensation to VCC supply.

R52 → 1 kΩ
C87 → 470 pF
C88 → 47 µF

BOM (for 1 board):

|  |  |  |  |
| --- | --- | --- | --- |
| **Qty** | **Item** | **Distributor** | **Description** |
| 3 | 399-C0805C471J5GAC7210CT-ND | Digi-Key | C112/C113/C87, 470 pF |
| 2 | RR1220Q-150-D | Digi-Key | R69/R70, 15 Ω |
| 1 | P1.0KDACT-ND | Digi-Key | R52, 1 kΩ |
| 1 | 1276-3137-1-ND | Digi-Key | C88, 2.2 µF, 50V |
| 1 | 490-5528-1-ND | Digi-Key | C88, 47 µF, 10V |